{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Data entry","Instructions"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data entry","index":0,"n_rows":20,"n_cols":8,"rows_kept":20,"cut":false,"hidden":false,"merged":[[12,0,12,6],[14,0,14,6],[5,0,5,8],[3,1,3,7],[6,1,6,3],[13,2,13,6],[15,2,15,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6]]}
[]
[]
[]
[null,"Enter Laboratory or Organization Name"]
[]
["Conversion Data Entry Page"]
[]
[]
[null,null,"Enter Fahrenheit degrees to convert to Celsius degrees: "]
[null,null,"Equivalent Celsius degrees: ",null,null,null,null,{"$f":"IF(H9=\"\",\"\",H9*5/9)","v":""}]
[null,null,"Enter Celsius degrees to convert to Fahrenheit  degrees: "]
[null,null,"Equivalent Fahrenheit degrees: ",null,null,null,null,{"$f":"IF(H11=\"\",\"\",H11*1.8)","v":""}]
["Enter Fahrenheit temperature to convert to Celsius temperature: "]
[null,null,"Equivalent Celsius temperature: ",null,null,null,null,{"$f":"IF(H13=\"\",\"\",(H13-32)*5/9)","v":""}]
["Enter Celsius temperature to convert to Fahrenheit temperature: "]
[null,null,"Equivalent Fahrenheit temperature: ",null,null,null,null,{"$f":"IF(H15=\"\",\"\",(H15*9/5)+32)","v":""}]
[]
[]
[null,null,null,null,null,null,null,"Spreadsheet created by:"]
[null,null,null,null,null,null,null,"Henry L. Alexander CMfgE CQE"]

{"sheet":"Instructions","index":1,"n_rows":32,"n_cols":20,"rows_kept":32,"cut":false,"hidden":false,"merged":[[23,0,23,1],[21,1,21,7],[22,1,22,7],[20,1,20,7],[18,1,18,6],[16,1,16,7],[17,1,17,7],[19,1,19,7],[12,1,12,7],[13,1,13,6],[14,1,14,7],[1,0,1,7],[3,1,3,6],[5,1,5,7],[4,1,4,6],[11,1,11,6],[6,1,6,6],[10,1,10,6]]}
[]
[{"$f":"'Data entry'!$B$4","v":"Enter Laboratory or Organization Name"}]
[]
[null,"To convert a number of degrees:"]
[1,"Enter a number of Fahrenheit degrees to convert to the equivilant Celsius degrees"]
[2,"Enter a number of Celsius  degrees to convert to the equivilant Fahrenheit degrees",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CMC"]
[null,"The following formula are used In making the conversions:"]
[null,"1 C° = 5/9 F°"]
[null,"1 F° = 9/5 C°"]
[]
[null,"To convert a temperature from one system of units to another:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Select budget type"]
[1,"Enter a number of Fahrenheit degrees to convert to the equivilant Celsius degrees",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Budget for Estimation of Uncertainty of Measurement "]
[2,"Enter a number of Celsius  degrees to convert to the equivilant Fahrenheit degrees",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Budget for Estimation of Calibration and Measurement Capability (CMC) "]
[null,"The following formula are used In making the conversions:"]
[null,"Temperature in °C = (Temperature in °F - 32) * 5/9",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"   Select"]
[null,"Temperature in °F= (Temperature in °C * 9/5) + 32",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Unc"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CMC"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"µin/in/°F"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"µ"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"°"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12.3]
["Ver LS-04"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Unc",null,"CMC"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.4999999999999997E-2,null,3.7499999999999999E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6.5,null,6.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4.4000000000000004,null,4.4000000000000004]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(R30+R29*R30)-(R31-R29*R31)","v":2.9174999999999995},null,{"$f":"(T30+T29*T30)-(T31-T29*T31)","v":2.50875}]