{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["dBm to Watt Converter"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"dBm to Watt Converter","index":0,"n_rows":30,"n_cols":10,"rows_kept":30,"cut":false,"hidden":false,"merged":[[13,7,13,8],[19,7,19,8],[3,6,4,9]]}
[]
[]
[]
[null,null,null,null,null,null,"Convert dBm to equivilant Watts"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Power Conversion (Watts to dBm)"]
[null,null,null,null,null,null,null,"Stated Power","Equivilant dBm"]
[null,null,null,null,null,null,null,null,{"$f":"IF(H16=\"\",\"\",10*LOG10(1000*H16))","v":""}]
[]
[]
[]
[null,null,null,null,null,null,null,"Power Conversion (dBm to Watts)"]
[null,null,null,null,null,null,null,"dBm","Equivilant Watts"]
[null,null,null,null,null,null,null,null,{"$f":"IF(H22=\"\",\"\",(10^(H22/10))/1000)","v":""}]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,"Spreadsheet created by:"]
[null,null,null,null,null,null,null,null,null,"Henry L. Alexander CMfgE CQE"]